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	CYCLE TYRE SEAL
	Tömlö töltő aerosolos 100ml. 3010

	DIRECTIONS: For temporary puncture repairs.

Remove object causing puncture. Shake can well. If cold, warm in hands. With tyre valve at 12 o’clock position, screw connector onto valve use adaptor if required and re-inflate. Cycle immediately to spread sealant. Repair permanently as soon as possible.
	

	CAUTION:
	VIGYÁZAT:

	Extremely Flammable.
	Fokozottan tűzveszélyes.

	Harmful to aquatic organisms, may cause long-term adverse effects in the aquatic environment.
	Ártalmas a vízi szervezetekre, a vízi környezetben hosszan tartó károsodást okozhat.

	Keep out of reach of children.
	Gyermekek kezébe nem kerülhet

	Keep away from sources of ignition - No smoking.
	Gyújtóforrástól távol tartandó - Tilos a dohányzás

	Do not breathe spray.
	A keletkező permetet nem szabad belélegezni.

	Pressurised Container. Protect from sunlight. Do not expose to temperatures above 50ºC.
	A tartály túlnyomás alatt áll: napfénytől elzárva és 50 °C-ot meg nem haladó hőmérsékleten tárolandó. 

	Do not spray on flame or incandescent materials.
	Tilos nyílt lángba vagy izzó anyagra porlasztani.

	Do not pierce or burn, even after use.
	Kilyukasztani, tűzbe dobni használat után is tilos.


